CMSIS-DAP: DAP_SWJ_Clock

| CMSIS-DAP Version 2.0.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_SWJ_Clock
Common SWD/JTAG Commands

Select SWD/JTAG Clock. More...

Select SWD/JTAG Clock.

The DAP_SWJ_Clock Command sets the clock frequency for JTAG and SWD communication mode.

DAP_SWJ_Clock Command:

| BYTE | WORD *|
> 0x11 | Clock |
|******|*******|

- Clock: Selects maximum SWD/JTAG Clock (SWCLK/TCK) value in Hz

DAP_SWJ_Clock Response:

| BYTE | BYTE **|
< 0x11 | Status |
|******|********|

- Status: Response Status