CMSIS-Zone (Preview): /azone/zones element

| CMSIS-Zone (Preview) Version 0.9.2 System Resource Management

- Main Page
- Usage and Description

All Files Pages
/azone/zones element

The /azone/zones element contains all zone definitions.

Example

<zones>
<zone name="Network">
<assign region="RAM1" block="Network" access="rw"/>
<assign group="UART" peripheral="USART0" access="rw" />
:
</zone>
:
</zones>

Parent Element | Element Chain
--- | ---
azone | /azone element
Child Elements | Description | Type | Occurrence
zone | Zone definitions | complexType | 1..*

# /azone/zones/zone element

The /azone/zones/zone element defines the name of a zone.

Parent Element | Element Chain
--- | ---
zones | /azone/zones element
Attributes | Description | Type | Use
name | The unique name for this zone. | xs:string | required
info | Brief description of the zone. | xs:string | optional
Pname | The processor that can access the memory and peripherals of this zone. If omitted all processors of the system have access. | xs:string | optional
security | Security level for code execution in this zone. | SecurityType | optional
privilege | Privilege level for code execution in this zone. | PrivilegeType | optional
Child Elements | Description | Type | Occurrence
assign | Resource Assignments | complexType | 1..*

# /azone/zones/zone/assign element

The /azone/zones/zone/assign element defines the resource assignments of that zone.

Parent Element | Element Chain
--- | ---
zone | /azone/zones/zone element
Attributes | Description | Type | Use
memory | Name of a memory region or memory partition. | xs:string | optional
group | Name of a peripheral group. | xs:string | optional
peripheral | Name of a peripheral. | xs:string | optional
access | Access permissions for this assignment. | AccessType | optional
Pname | The processor that can access this assignment. If omitted the processors of the zone have access. | xs:string | optional
security | Security attributes for this assignment. | SecurityType | optional
privilege | Privilege level for this assignment. | PrivilegeType | optional
uninit | "1" specifies that this region is not zero initialized during startup. Default value is "0". | xs:boolean | optional
dma | "1" specifies that this region is accessed by a DMA controller. Default value is "0". | xs:boolean | optional
Child Elements | Description | Type | Occurrence
interrupt | Interrupt assignments for peripherals. | complexType | 0..*

# /azone/zones/zone/assign/interrupt element

The /azone/zones/zone/assign/interrupt element defines the interrupt execution for a peripheral.

Parent Element | Element Chain
--- | ---
assign | /azone/zones/zone/assign element
Attributes | Description | Type | Use
name | The name of the interrupt. | xs:string | required
value | The interrupt number. | xs:string | required
info | Brief description for this setting. | xs:string | optional
security | Security setting for the interrupt. | SecurityType | optional
privilege | Privilege level setting for the interrupt. | PrivilegeType | optional