CMSIS-Driver: Ethernet MAC Control Codes

| CMSIS-Driver Version 2.7.1 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content
Ethernet MAC Control Codes
Ethernet MAC Interface

Configure and control the Ethernet MAC using the ARM_ETH_MAC_Control. More...

## Content
| Ethernet MAC Controls
| Configure and control the Ethernet MAC interface.
| Ethernet MAC Configuration
| Specifies speed mode, link mode, checksum, and frame filtering modes.
| Ethernet MAC Flush Flags
| Specify controls to flush a buffer.
| Ethernet MAC VLAN Filter Flag
| Specify whether to compare only the VLAN Identifier.

## Description

Configure and control the Ethernet MAC using the ARM_ETH_MAC_Control.

Many parameters of the Ethernet MAC driver are configured using the ARM_ETH_MAC_Control function.

The various Ethernet MAC control codes define:

- Ethernet MAC Controls configures and controls the Ethernet MAC interface
- Ethernet MAC Configuration specifies speed mode, link mode, checksum, and frame filtering modes
- Ethernet MAC Flush Flags specify controls to flush a buffer
- Ethernet MAC VLAN Filter Flag specifies whether to compare only the VLAN Identifier

Refer to the ARM_ETH_MAC_Control function for further details.