CMSIS-RTOS2: Kernel Information and Control

| CMSIS-RTOS2 Version 2.1.3 Real-Time Operating System: API and RTX Reference Implementation

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Enumerations | Functions
Kernel Information and Control
CMSIS-RTOS API v2

Provides version/system information and starts/controls the RTOS Kernel. More...

## Data Structures
struct | osVersion_t
| Version information. More...

## Enumerations
enum | osKernelState_t { osKernelInactive = 0, osKernelReady = 1, osKernelRunning = 2, osKernelLocked = 3, osKernelSuspended = 4, osKernelError = -1, osKernelReserved = 0x7FFFFFFFU }
| Kernel state. More...

## Functions
osStatus_t | osKernelInitialize (void)
| Initialize the RTOS Kernel. More...
osStatus_t | osKernelGetInfo (osVersion_t *version, char *id_buf, uint32_t id_size)
| Get RTOS Kernel Information. More...
osKernelState_t | osKernelGetState (void)
| Get the current RTOS Kernel state. More...
osStatus_t | osKernelStart (void)
| Start the RTOS Kernel scheduler. More...
int32_t | osKernelLock (void)
| Lock the RTOS Kernel scheduler. More...
int32_t | osKernelUnlock (void)
| Unlock the RTOS Kernel scheduler. More...
int32_t | osKernelRestoreLock (int32_t lock)
| Restore the RTOS Kernel scheduler lock state. More...
uint32_t | osKernelSuspend (void)
| Suspend the RTOS Kernel scheduler. More...
void | osKernelResume (uint32_t sleep_ticks)
| Resume the RTOS Kernel scheduler. More...
uint32_t | osKernelGetTickCount (void)
| Get the RTOS kernel tick count. More...
uint32_t | osKernelGetTickFreq (void)
| Get the RTOS kernel tick frequency. More...
uint32_t | osKernelGetSysTimerCount (void)
| Get the RTOS kernel system timer count. More...
uint32_t | osKernelGetSysTimerFreq (void)
| Get the RTOS kernel system timer frequency. More...

## Description

The kernel Information and Control function group allows to:

- obtain information about the system and the underlying kernel.
- obtain version information about the CMSIS-RTOS API.
- initialize of the RTOS kernel for creating objects.
- start the RTOS kernel and thread switching.
- check the execution status of the RTOS kernel.

Note
  The kernel information and control functions cannot be called from Interrupt Service Routines.
  The kernel initialization for RTX5 is documented in System Startup.

Code Example

/*----------------------------------------------------------------------------
* Application main thread
*---------------------------------------------------------------------------*/
void app_main (void *argument) {
// ...
for (;;) {}
}
int main (void) {
// System Initialization
SystemCoreClockUpdate();
// ...
osKernelInitialize(); // Initialize CMSIS-RTOS
osThreadNew(app_main, NULL, NULL); // Create application main thread
osKernelStart(); // Start thread execution
for (;;) {}
}

## Data Structure Documentation

struct osVersion_t

Identifies the underlying RTOS kernel and API version number. The version is represented in a combined decimal number in the format: major.minor.rev: mmnnnrrrr

Use osKernelGetInfo to retrieve the version numbers.

Data Fields
uint32_t | api | API version (major.minor.rev: mmnnnrrrr dec).
uint32_t | kernel | Kernel version (major.minor.rev: mmnnnrrrr dec).

## Enumeration Type Documentation

enum osKernelState_t

State of the kernel as retrieved by osKernelGetState. In case osKernelGetState fails or if it is called from an ISR, it will return `osKernelError`, otherwise it returns the kernel state.

Enumerator
osKernelInactive | Inactive. The kernel is not ready yet. osKernelInitialize needs to be executed successfully.
osKernelReady | Ready. The kernel is not yet running. osKernelStart transfers the kernel to the running state.
osKernelRunning | Running. The kernel is initialized and running.
osKernelLocked | Locked. The kernel was locked with osKernelLock. The functions osKernelUnlock or osKernelRestoreLock unlocks it.
osKernelSuspended | Suspended. The kernel was suspended using osKernelSuspend. The function osKernelResume returns to normal operation.
osKernelError | Error. An error occurred.
osKernelReserved | Prevents enum down-size compiler optimization. Reserved.

## Function Documentation

osStatus_t osKernelInitialize | ( | void |  | ) |

Returns
  status code that indicates the execution status of the function.

The function osKernelInitialize initializes the RTOS Kernel. Before it is successfully executed, only the functions osKernelGetInfo and osKernelGetState may be called.

Possible osStatus_t return values:

- osOK in case of success.
- osError if an unspecific error occurred.
- osErrorISR if called from an Interrupt Service Routine.
- osErrorNoMemory if no memory could be reserved for the operation.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

#include "RTE_Components.h"
#include CMSIS_device_header
#include "cmsis_os2.h"
/*----------------------------------------------------------------------------
* Application main thread
*---------------------------------------------------------------------------*/
void app_main (void *argument) {
// ...
for (;;) {}
}
int main (void) {
// System Initialization
SystemCoreClockUpdate();
// ...
osKernelInitialize(); // Initialize CMSIS-RTOS
osThreadNew(app_main, NULL, NULL); // Create application main thread
osKernelStart(); // Start thread execution
for (;;) {}
}

osStatus_t osKernelGetInfo | ( | osVersion_t * | version,
|  | char * | id_buf,
|  | uint32_t | id_size
| ) |  |

Parameters

  [out] | version | pointer to buffer for retrieving version information.
  [out] | id_buf | pointer to buffer for retrieving kernel identification string.
  [in] | id_size | size of buffer for kernel identification string.

Returns
  status code that indicates the execution status of the function.

The function osKernelGetInfo retrieves the API and kernel version of the underlying RTOS kernel and a human readable identifier string for the kernel. It can be safely called before the RTOS is initialized or started (call to osKernelInitialize or osKernelStart).

Possible osStatus_t return values:

- osOK in case of success.
- osError if an unspecific error occurred.

Note
  This function may be called from Interrupt Service Routines.

Code Example

void info (void) {
char infobuf[100];
osVersion_t osv;
osStatus_t status;
status = osKernelGetInfo(&osv, infobuf, sizeof(infobuf));
if(status == osOK) {
printf("Kernel Information: %s\r\n", infobuf);
printf("Kernel Version : %d\r\n", osv.kernel);
printf("Kernel API Version: %d\r\n", osv.api);
}
}

osKernelState_t osKernelGetState | ( | void |  | ) |

Returns
  current RTOS Kernel state.

The function osKernelGetState returns the current state of the kernel and can be safely called before the RTOS is initialized or started (call to osKernelInitialize or osKernelStart). In case it fails it will return `osKernelError`, otherwise it returns the kernel state (refer to osKernelState_t for the list of kernel states).

Possible osKernelState_t return values:

- osKernelError if an unspecific error occurred.
- the actual kernel state otherwise.

Note
  This function may be called from Interrupt Service Routines.

Code Example

int main (void) {
// System Initialization
SystemCoreClockUpdate();
// ...
if(osKernelGetState() == osKernelInactive) { // Is the kernel initialized?
osKernelInitialize(); // Initialize CMSIS-RTOS kernel
}
;
}

osStatus_t osKernelStart | ( | void |  | ) |

Returns
  status code that indicates the execution status of the function.

The function osKernelStart starts the RTOS kernel and begins thread switching. It will not return to its calling function in case of success. Before it is successfully executed, only the functions osKernelGetInfo, osKernelGetState, and object creation functions (osXxxNew) may be called.

At least one initial thread should be created prior osKernelStart, see osThreadNew.

Possible osStatus_t return values:

- osError if an unspecific error occurred.
- osErrorISR if called from an Interrupt Service Routine.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

int main (void) {
// System Initialization
SystemCoreClockUpdate();
// ...
if(osKernelGetState() == osKernelInactive) {
osKernelInitialize();
}
; // ... Start Threads
if (osKernelGetState() == osKernelReady) { // If kernel is ready to run...
osKernelStart(); // ... start thread execution
}
while(1); // only reached in case of error
}

int32_t osKernelLock | ( | void |  | ) |

Returns
  previous lock state (1 - locked, 0 - not locked, error code if negative).

The function osKernelLock allows to lock all task switches. It returns the previous value of the lock state (1 if it was locked, 0 if it was unlocked), or a negative number representing an error code otherwise (refer to osStatus_t).

Possible osStatus_t return values:

- osError if an unspecific error occurred.
- osErrorISR if called from an Interrupt Service Routine.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

int32_t state = osKernelLock();
// ... critical code
osKernelRestore(state);

int32_t osKernelUnlock | ( | void |  | ) |

Returns
  previous lock state (1 - locked, 0 - not locked, error code if negative).

The function osKernelUnlock resumes from osKernelLock. It returns the previous value of the lock state (1 if it was locked, 0 if it was unlocked), or a negative number representing an error code otherwise (refer to osStatus_t).

Possible osStatus_t return values:

- osError if an unspecific error occurred.
- osErrorISR if called from an Interrupt Service Routine.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

int32_t sl = osKernelLock();
// ... critical code
{
int32_t su = osKernelUnlock();
// ... uncritical code
osKernelRestoreLock(su);
}
// ... critical code
osKernelRestoreLock(sl);

int32_t osKernelRestoreLock | ( | int32_t | lock | ) |

Parameters

  [in] | lock | lock state obtained by osKernelLock or osKernelUnlock.

Returns
  new lock state (1 - locked, 0 - not locked, error code if negative).

The function osKernelRestoreLock restores the previous lock state after osKernelLock or osKernelUnlock.

The argument lock specifies the lock state as obtained by osKernelLock or osKernelUnlock.

The function returns the new value of the lock state (1 if it was locked, 0 if it was unlocked), or a negative number representing an error code otherwise (refer to osStatus_t).

Possible osStatus_t return values:

- osError if an unspecific error occurred.
- osErrorISR if called from an Interrupt Service Routine.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

int32_t sl = osKernelLock();
// ... critical code
{
int32_t su = osKernelUnlock();
// ... uncritical code
osKernelRestoreLock(su);
}
// ... critical code
osKernelRestoreLock(sl);

uint32_t osKernelSuspend | ( | void |  | ) |

Returns
  time in ticks, for how long the system can sleep or power-down.

CMSIS-RTOS provides extension for tick-less operation which is useful for applications that use extensively low-power modes where the SysTick timer is also disabled. To provide a time-tick in such power-saving modes a wake-up timer is used to derive timer intervals. The function osKernelSuspend suspends the RTX kernel scheduler and thus enables sleep modes.

The return value can be used to determine the amount of system ticks until the next tick-based kernel event will occure, i.e. a delayed thread becomed ready again. It is recommended to set up the low power timer to generate a wake-up interrupt based on this return value.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

void osRtxIdleThread (void) {
/* The idle thread is running
when no other thread is ready
to run. */
unsigned int sleep;
for (;;) {
/* HERE: include optional user
code to be executed when no
task runs. */
sleep = osKernelSuspend(); /* Suspend RTX thread scheduler */
if (sleep) { /* How long can we sleep? */
/* "sleep" is in RTX Timer Ticks
which is 1ms in this
configuration */
/* Setup wake-up e.g. watchdog */
__WFE(); /* Enter Power-down mode */
/* After Wake-up */
sleep = tc; /* Adjust with cycles slept */
}
osKernelResume(sleep); /* Resume thread scheduler */
}
}

void osKernelResume | ( | uint32_t | sleep_ticks | ) |

Parameters

  [in] | sleep_ticks | time in ticks for how long the system was in sleep or power-down mode.

CMSIS-RTOS provides extension for tick-less operation which is useful for applications that use extensively low-power modes where the SysTick timer is also disabled. To provide a time-tick in such power-saving modes a wake-up timer is used to derive timer intervals. The function osKernelResume enables the RTX kernel scheduler and thus wakes up the system from sleep mode.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

void osRtxIdleThread (void) {
/* The idle thread is running
when no other thread is ready
to run. */
unsigned int sleep;
for (;;) {
/* HERE: include optional user
code to be executed when no
task runs. */
sleep = osKernelSuspend(); /* Suspend RTX thread scheduler */
if (sleep) { /* How long can we sleep? */
/* "sleep" is in RTX Timer Ticks
which is 1ms in this
configuration */
/* Setup wake-up e.g. watchdog */
__WFE(); /* Enter Power-down mode */
/* After Wake-up */
sleep = tc; /* Adjust with cycles slept */
}
osKernelResume(sleep); /* Resume thread scheduler */
}
}

uint32_t osKernelGetTickCount | ( | void |  | ) |

Returns
  RTOS kernel current tick count.

The function osKernelGetTickCount returns the current RTOS kernel tick count.

Note
  This function may be called from Interrupt Service Routines.

Code Example

#include "cmsis_os2.h"
void Thread_1 (void *arg) { // Thread function
uint32_t tick;
tick = osKernelGetTickCount(); // retrieve the number of system ticks
for (;;) {
tick += 1000; // delay 1000 ticks periodically
osDelayUntil(tick);
// ...
}
}

Due to the limited value range used for the tick count it may overflow during runtime, i.e. after 232 ticks which are roughly 49days @ 1ms. Typically one has not to take special care of this unless a monotonic counter is needed. For such a case an additional 64bit tick counter can be implemented as follows. The given example needs GetTick() called at least twice per tick overflow to work properly.

Code Example

uint64_t GetTick(void) {
static uint32_t tick_h = 0U;
static uint32_t tick_l = 0U;
uint32_t tick;
tick = osKernelGetTickCount();
if (tick < tick_l) {
tick_h++;
}
tick_l = tick;
return (((uint64_t)tick_h << 32) | tick_l);
}

uint32_t osKernelGetTickFreq | ( | void |  | ) |

Returns
  frequency of the kernel tick in hertz, i.e. kernel ticks per second.

The function osKernelGetTickFreq returns the frequency of the current RTOS kernel tick.

Note
  This function may be called from Interrupt Service Routines.

uint32_t osKernelGetSysTimerCount | ( | void |  | ) |

Returns
  RTOS kernel current system timer count as 32-bit value.

The function osKernelGetSysTimerCount returns the current RTOS kernel system timer as a 32-bit value.

Note
  This function may be called from Interrupt Service Routines.

uint32_t osKernelGetSysTimerFreq | ( | void |  | ) |

Returns
  frequency of the system timer in hertz, i.e. timer ticks per second.

The function osKernelGetSysTimerFreq returns the frequency of the current RTOS kernel system timer.

Note
  This function may be called from Interrupt Service Routines.