CMSIS-Core (Cortex-A): PL1 Physical Timer Control register (CNTP_CTL)

| CMSIS-Core (Cortex-A) Version 1.1.4 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
PL1 Physical Timer Control register (CNTP_CTL)
Core Register Access

The control register for the physical timer. More...

## Functions
__STATIC_FORCEINLINE void | __set_CNTP_CTL (uint32_t value)
| Set CNTP_CTL. More...
__STATIC_FORCEINLINE uint32_t | __get_CNTP_CTL (void)
| Get CNTP_CTL register. More...

## Description

Bits | Name | Function
--- | --- | ---
[31:3] | - | Reserved.
[2] | ISTATUS | The status of the timer.
[1] | IMASK | Timer output signal mask bit.
[0] | ENABLE | Enables the timer.

Consider __get_CNTP_CTL and __set_CNTP_CTL to access this register.

Consider using Generic Physical Timer Functions for controlling the PL1 Timer instead.

## Function Documentation

__STATIC_INLINE uint32_t __get_CNTP_CTL | ( | void |  | ) |

Returns
  CNTP_CTL Register value

This function returns the value of the PL1 Physical Timer Control Register. (CNTP_CTL).

__STATIC_INLINE void __set_CNTP_CTL | ( | uint32_t | value | ) |

This function assigns the given value to PL1 Physical Timer Control Register (CNTP_CTL).

Parameters

  [in] | value | CNTP_CTL Register value to set

This function assigns the given value to PL1 Physical Timer Control Register (CNTP_CTL).