CMSIS-Core (Cortex-A): ACTLR_Type Struct Reference

| CMSIS-Core (Cortex-A) Version 1.1.4 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
ACTLR_Type Struct Reference
Auxiliary Control Register (ACTLR)

Bit field declaration for ACTLR layout.

## Data Fields
struct {
uint32_t FW:1
| bit: 0 Cache and TLB maintenance broadcast More...
uint32_t SMP:1
| bit: 6 Enables coherent requests to the processor More...
uint32_t EXCL:1
| bit: 7 Exclusive L1/L2 cache control More...
uint32_t DODMBS:1
| bit: 10 Disable optimized data memory barrier behavior More...
uint32_t DWBST:1
| bit: 11 AXI data write bursts to Normal memory More...
uint32_t RADIS:1
| bit: 12 L1 Data Cache read-allocate mode disable More...
uint32_t L1PCTL:2
| bit:13..14 L1 Data prefetch control More...
uint32_t BP:2
| bit:16..15 Branch prediction policy More...
uint32_t RSDIS:1
| bit: 17 Disable return stack operation More...
uint32_t BTDIS:1
| bit: 18 Disable indirect Branch Target Address Cache (BTAC) More...
uint32_t DBDI:1
| bit: 28 Disable branch dual issue More...
} | b
| Structure used for bit access on Cortex-A5. More...
struct {
uint32_t SMP:1
| bit: 6 Enables coherent requests to the processor More...
uint32_t DODMBS:1
| bit: 10 Disable optimized data memory barrier behavior More...
uint32_t L2RADIS:1
| bit: 11 L2 Data Cache read-allocate mode disable More...
uint32_t L1RADIS:1
| bit: 12 L1 Data Cache read-allocate mode disable More...
uint32_t L1PCTL:2
| bit:13..14 L1 Data prefetch control More...
uint32_t DDVM:1
| bit: 15 Disable Distributed Virtual Memory (DVM) transactions More...
uint32_t DDI:1
| bit: 28 Disable dual issue More...
} | b
| Structure used for bit access on Cortex-A7. More...
struct {
uint32_t FW:1
| bit: 0 Cache and TLB maintenance broadcast More...
uint32_t L1PE:1
| bit: 2 Dside prefetch More...
uint32_t WFLZM:1
| bit: 3 Cache and TLB maintenance broadcast More...
uint32_t SMP:1
| bit: 6 Enables coherent requests to the processor More...
uint32_t EXCL:1
| bit: 7 Exclusive L1/L2 cache control More...
uint32_t AOW:1
| bit: 8 Enable allocation in one cache way only More...
uint32_t PARITY:1
| bit: 9 Support for parity checking, if implemented More...
} | b
| Structure used for bit access on Cortex-A9. More...
uint32_t | w
| Type used for word access. More...

## Field Documentation

uint32_t ACTLR_Type::AOW

struct { ... } ACTLR_Type::b

struct { ... } ACTLR_Type::b

struct { ... } ACTLR_Type::b

uint32_t ACTLR_Type::BP

uint32_t ACTLR_Type::BTDIS

uint32_t ACTLR_Type::DBDI

uint32_t ACTLR_Type::DDI

uint32_t ACTLR_Type::DDVM

uint32_t ACTLR_Type::DODMBS

uint32_t ACTLR_Type::DWBST

uint32_t ACTLR_Type::EXCL

uint32_t ACTLR_Type::FW

uint32_t ACTLR_Type::L1PCTL

uint32_t ACTLR_Type::L1PE

uint32_t ACTLR_Type::L1RADIS

uint32_t ACTLR_Type::L2RADIS

uint32_t ACTLR_Type::PARITY

uint32_t ACTLR_Type::RADIS

uint32_t ACTLR_Type::RSDIS

uint32_t ACTLR_Type::SMP

uint32_t ACTLR_Type::w

uint32_t ACTLR_Type::WFLZM