CMSIS-Core (Cortex-A): GICInterface_Type Struct Reference

| CMSIS-Core (Cortex-A) Version 1.1.4 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
GICInterface_Type Struct Reference
Generic Interrupt Controller Functions

Structure type to access the Generic Interrupt Controller Interface (GICC)

## Data Fields
__IOM uint32_t | CTLR
| Offset: 0x000 (R/W) CPU Interface Control Register. More...
__IOM uint32_t | PMR
| Offset: 0x004 (R/W) Interrupt Priority Mask Register. More...
__IOM uint32_t | BPR
| Offset: 0x008 (R/W) Binary Point Register. More...
__IM uint32_t | IAR
| Offset: 0x00C (R/ ) Interrupt Acknowledge Register. More...
__OM uint32_t | EOIR
| Offset: 0x010 ( /W) End Of Interrupt Register. More...
__IM uint32_t | RPR
| Offset: 0x014 (R/ ) Running Priority Register. More...
__IM uint32_t | HPPIR
| Offset: 0x018 (R/ ) Highest Priority Pending Interrupt Register. More...
__IOM uint32_t | ABPR
| Offset: 0x01C (R/W) Aliased Binary Point Register. More...
__IM uint32_t | AIAR
| Offset: 0x020 (R/ ) Aliased Interrupt Acknowledge Register. More...
__OM uint32_t | AEOIR
| Offset: 0x024 ( /W) Aliased End Of Interrupt Register. More...
__IM uint32_t | AHPPIR
| Offset: 0x028 (R/ ) Aliased Highest Priority Pending Interrupt Register. More...
__IOM uint32_t | STATUSR
| Offset: 0x02C (R/W) Error Reporting Status Register, optional. More...
__IOM uint32_t | APR [4]
| Offset: 0x0D0 (R/W) Active Priority Register. More...
__IOM uint32_t | NSAPR [4]
| Offset: 0x0E0 (R/W) Non-secure Active Priority Register. More...
__IM uint32_t | IIDR
| Offset: 0x0FC (R/ ) CPU Interface Identification Register. More...
__OM uint32_t | DIR
| Offset: 0x1000( /W) Deactivate Interrupt Register. More...

## Field Documentation

__IOM uint32_t GICInterface_Type::ABPR

CPU Interface Aliased Binary Point Register

See Also
  GICInterface_Type::BPR

__OM uint32_t GICInterface_Type::AEOIR

CPU Interface Aliased End Of Interrupt Register

See Also
  GICInterface_Type::EOIR

__IM uint32_t GICInterface_Type::AHPPIR

CPU Interface Aliased Highest Priority Pending Interrupt Register

See Also
  GICInterface_Type::HPPIR

__IM uint32_t GICInterface_Type::AIAR

CPU Interface Aliased Interrupt Acknowledge Register

See Also
  GICInterface_Type::IAR

__IOM uint32_t GICInterface_Type::APR[4]

CPU Interface Active Priorities Registers

Note
  The register values are IMPLEMENTATION DEFINED.

__IOM uint32_t GICInterface_Type::BPR

CPU Interface Binary Point Register

Bits | Name | Function
--- | --- | ---
[31:3] | - | Reserved.
[2:0] | Binary_Point | Controls how the 8-bit interrupt priority field is split into a group priority field and a subpriority field.

The binary point (values 0-7) defines the amount of priority bits used as subpriority. Please refer to the section Interrupt prioritization in the Arm Generic Interrupt Controller Architecture Specificaton for details.

__IOM uint32_t GICInterface_Type::CTLR

CPU Interface Control Register

Enables the signaling of interrupts by the CPU interface to the connected processor, and provides additional top-level control of the CPU interface. In a GICv2 implementation, this includes control of the end of interrupt (EOI) behavior.

Bits | Name | Function
--- | --- | ---
[31:1] | - | Reserved.
[0] | Enable | Interrupt signaling: 0 - Disable. 1 - Enable.

__OM uint32_t GICInterface_Type::DIR

CPU Interface Deactivate Interrupt Register

Bits | Name | Function
--- | --- | ---
[31:24] | - | Reserved.
[23:0] | INTID | The INTID of the interrupt to be disabled.

__OM uint32_t GICInterface_Type::EOIR

CPU Interface End Of Interrupt Register

Bits | Name | Function
--- | --- | ---
[31:24] | - | Reserved.
[23:0] | INTID | The interrupt number of the finished interrupt.

__IM uint32_t GICInterface_Type::HPPIR

CPU Interface Highest Priority Pending Interrupt Register

Bits | Name | Function
--- | --- | ---
[31:24] | - | Reserved.
[23:0] | INTID | The INTID of the signaled interrupt.

__IM uint32_t GICInterface_Type::IAR

CPU Interface Interrupt Acknowledge Register

Bits | Name | Function
--- | --- | ---
[31:24] | - | Reserved.
[23:0] | INTID | The interrupt number of the signaled interrupt.

__IM uint32_t GICInterface_Type::IIDR

CPU Interface Identification Register

Bits | Name | Function
--- | --- | ---
[31:20] | ProductID | An IMPLEMENTATION DEFINED product identifier
[19:16] | Arch_version | The version of the GIC architecture that is implemented.
[15:12] | Revision | An IMPLEMENTATION DEFINED revision number for the CPU interface.
[11:0] | Implementer | Contains the JEP106 code of the company that implemented the CPU interface.

__IOM uint32_t GICInterface_Type::NSAPR[4]

CPU Interface Non-secure Active Priorities Registers

Note
  The register values are IMPLEMENTATION DEFINED.

See Also
  GICInterface_Type::APR[4]

__IOM uint32_t GICInterface_Type::PMR

CPU Interface Priority Mask Register

Bits | Name | Function
--- | --- | ---
[31:8] | - | Reserved.
[7:0] | Priority | The priority mask level for the CPU interface.

Note
  IMPLEMENTATION DEFINED unsupported priority bits might be RAZ/WI.

__IM uint32_t GICInterface_Type::RPR

CPU Interface Running Priority Register

Bits | Name | Function
--- | --- | ---
[31:8] | - | Reserved.
[7:0] | Priority | The current running priority on the CPU interface.

__IOM uint32_t GICInterface_Type::STATUSR

CPU Interface Status Register

Bits | Name | Function
--- | --- | ---
[31:5] | - | Reserved.
[4] | ASV | Attempted security violation.
[3] | WROD | Write to an RO location.
[2] | RWOD | Read of a WO location.
[1] | WRD | Write to a reserved location.
[0] | RRD | Read of a reserved location.