CMSIS-Driver: Revision History of CMSIS-Driver

| CMSIS-Driver Version 2.7.1 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Revision History of CMSIS-Driver

Version | Description
--- | ---
2.7.1 | Modifications compared to Version 2.7.0: Finalized WiFi Interface API 1.0.0.
2.7.0 | Modifications compared to Version 2.6.0: Added WiFi Interface API 1.0.0-beta. Added custom driver selection to simplify implementation of new CMSIS-Driver.
2.6.0 | Modifications compared to Version 2.05: Enhanced CAN-Driver API with explicit BUSOFF state. Enhanced NAND-Driver API for ECC handling.
2.05 | Modifications compared to Version 2.04: Changed: All typedefs related to status have been made volatile.
2.04 | Modifications compared to Version 2.03: Added: template files for CAN interface driver.
2.03 | Modifications compared to Version 2.02: Added: CAN API for an interface to CAN peripherals Added: Overview of the CMSIS-Driver Validation Software Pack. Enhanced: documentation and clarified behavior of the Function Call Sequence.
2.02 | Modifications compared to Version 2.00: Minor API changes, for exact details refer to the header file of each driver. Added: Flash Interface, NAND interface.
2.00 | API with non-blocking data transfer, independent of CMSIS-RTOS.
1.10 | Initial release