CMSIS-NN: arm_depthwise_conv_u8_basic_ver1.c File Reference

| CMSIS-NN Version 1.2.0 CMSIS NN Software Library

- Main Page
- Usage and Description
- Reference

All Data Structures Namespaces Files Functions Variables Enumerations Enumerator Macros Groups Pages
Macros | Functions
arm_depthwise_conv_u8_basic_ver1.c File Reference

## Macros
#define | DILATION_X
#define | DILATION_Y

## Functions
arm_status | arm_depthwise_conv_u8_basic_ver1 (const uint8_t *input, const uint16_t input_x, const uint16_t input_y, const uint16_t input_ch, const uint8_t *kernel, const uint16_t kernel_x, const uint16_t kernel_y, const int16_t ch_mult, const int16_t pad_x, const int16_t pad_y, const int16_t stride_x, const int16_t stride_y, const int16_t dilation_x, const int16_t dilation_y, const int32_t *bias, const int32_t input_offset, const int32_t filter_offset, const int32_t output_offset, uint8_t *output, const uint16_t output_x, const uint16_t output_y, const int32_t output_activation_min, const int32_t output_activation_max, const int32_t out_shift, const int32_t out_mult)
| uint8 depthwise convolution function with asymmetric quantization for even number of channel multiplier and input channels. Unless specified otherwise, arguments are mandatory. Both square and non-square inputs are accepted. More...

## Macro Definition Documentation

#define DILATION_X

Referenced by arm_depthwise_conv_u8_basic_ver1().

#define DILATION_Y

Referenced by arm_depthwise_conv_u8_basic_ver1().