CMSIS-NN: arm_nn_mat_mult_kernel_q7_q15.c File Reference

| CMSIS-NN Version 1.2.0 CMSIS NN Software Library

- Main Page
- Usage and Description
- Reference

All Data Structures Namespaces Files Functions Variables Enumerations Enumerator Macros Groups Pages
Functions
arm_nn_mat_mult_kernel_q7_q15.c File Reference

## Functions
q7_t * | arm_nn_mat_mult_kernel_q7_q15 (const q7_t *pA, const q15_t *pInBuffer, const uint16_t ch_im_out, const uint16_t numCol_A, const uint16_t bias_shift, const uint16_t out_shift, const q7_t *bias, q7_t *pOut)
| Matrix-multiplication function for convolution. More...

## Function Documentation

q7_t* arm_nn_mat_mult_kernel_q7_q15 | ( | const q7_t * | pA,
|  | const q15_t * | pInBuffer,
|  | const uint16_t | ch_im_out,
|  | const uint16_t | numCol_A,
|  | const uint16_t | bias_shift,
|  | const uint16_t | out_shift,
|  | const q7_t * | bias,
|  | q7_t * | pOut
| ) |  |

Matrix-Multiplication Kernels for Convolution.

Parameters

  [in] | pA | pointer to operand A
  [in] | pInBuffer | pointer to operand B, always conssists of 2 vectors
  [in] | ch_im_out | numRow of A
  [in] | numCol_A | numCol of A
  [in] | bias_shift | amount of left-shift for bias
  [in] | out_shift | amount of right-shift for output
  [in] | bias | the bias
  [in,out] | pOut | pointer to output

Returns
  The function returns the incremented output pointer

This function does the matrix multiplication with weight matrix and 2 columns from im2col.

References NN_ROUND.

Referenced by arm_convolve_HWC_q7_basic(), arm_convolve_HWC_q7_basic_nonsquare(), and arm_convolve_HWC_q7_RGB().