CMSIS-Core (Cortex-A): TLB maintenance operations

| CMSIS-Core (Cortex-A) Version 1.1.4 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
TLB maintenance operations
Core Register Access

This section describes the TLB operations that are implemented on all Armv7-A implementations. More...

## Functions
__STATIC_FORCEINLINE void | __set_TLBIALL (uint32_t value)
| Set TLBIALL. More...

## Description

TLB maintenance operations provide a mechanism to invalidate entries from a TLB.

Consider using Memory Management Unit Functions instead of raw register usage.

## Function Documentation

__STATIC_INLINE void __set_TLBIALL | ( | uint32_t | value | ) |

TLB Invalidate All

This function invalidates entire unified TLB.