CMSIS-Zone (Preview): mpc_setup[n] element

| CMSIS-Zone (Preview) Version 0.9.2 System Resource Management

- Main Page
- Usage and Description

All Files Pages
mpc_setup[n] element

The mpc_setup[n] element contains a sequence of device specific configuration for the setup of the Memory Protection Controller (MPC).

Parent Element | Element Chain
--- | ---
system | system element
Child Elements | Description | Type
.mpc_setup[n].name | The name of the base register that controls the MPC. | xs:string
.mpc_setup[n].memory | The name of the physical memory region that is connected via the MPC. | xs:string
.mpc_setup[n].blk_size | The block size information that CMSIS-Zone used for LUT generation. | NonNegativeInteger
.mpc_setup[n].S_bit[m] | A list of bit values for Secure attribute that are used to compose the LUT. | NonNegativeInteger
.mpc_setup[n].P_bit[m] | A list of bit values for Privileged attribute that are used to compose the LUT. | NonNegativeInteger
.mpc_setup[n].bits_comment[m] | The memory region information for source code comments that relate to S_bits or P_bits. | xs:string