CMSIS-Zone (Preview): /azone/configure element

| CMSIS-Zone (Preview) Version 0.9.2 System Resource Management

- Main Page
- Usage and Description

All Files Pages
/azone/configure element

The /azone/configure element allows to control the operation of the CMSIS-Zone utility.

Example

<configure mode="MPU"> // CMSIS-Zone utility UI behavior
<type name="RAM" hide="0" select="0" />
<type name="ROM" hide="1" select="1" />
<type name="Peripheral" hide="1" select="0" />
</configure>

Parent Element | Element Chain
--- | ---
azone | /azone element
Attributes | Description | Type | Use
mode | Operation mode ("Project" or "MPU") | xs:string | required
Child Elements | Description | Type | Occurrence
type | UI behavior for memory or peripheral selection depending on the operation mode | complexType | 0..*

# /azone/configure/type element

The /azone/configure/type element defines UI behavior of the CMSIS-Zone utility for a memory or peripheral selection depending on the operation mode.

Parent Element | Element Chain
--- | ---
configure | /azone/configure element
Attributes | Description | Type | Use
name | Refers item type ("RAM", "ROM", or "Peripheral") that this element specifies. | xs:string | required
hide | "1" specifies that the item type is hidden during configuration in the UI of the CMSIS-Zone utility (default is "0"). | xs:boolean | optional
select | "1" specifies that all resources with the item type are selected (default is "0"). | xs:boolean | optional